**Programmer’s Manual (MPX OS)**

1. **commhand():-**
   1. **Inputs:** none
   2. **Outputs:** none
   3. **Description:** Within Kernel, this function is called, which in return runs an endless loop to continuously ask the user for commands. This calls sys\_req(READ,…) which goes to polling for collecting inputs. It then uses strtok() to separate the commands into individual strings separated by spaces. Each command is processed and then the corresponding steps / lines of code are implemented.
   4. **Variables:**  
      int size: size of the command buffer  
      int sizeBuff: size of the time/date buffers  
      char buffer[]: the main command buffer  
      int dateBuff[] / int timeBuff[]: the buffers to store current date and time values.  
      char \*token: pointer to the first “word” in command buffer before a space  
      const char split[]: the character that splits the command buffer
2. **get\_Time(int \*pointer):-**
   1. **inputs:** a pointer to the time buffer
   2. **outputs:** none
   3. **macros:** 0x00 defined as Sec, 0x02 defined as Min and 0x04 defined as Hr.
   4. **Description:** Grabs the hours, minutes and seconds values from their respective RTC registers and fills them in the buffer given by the pointer. Because the values in the registers are stored in BCD form, they are first converted into binary form and then stored in the buffer one digit at a time.
3. **set\_Time(int hour, int minutes, int seconds):**-
   1. **Inputs:** int hours, int minutes, int seconds
   2. **Outputs:** none
   3. **Description:** Changes the current time of the machine to the provided values. This is achieved by converting each input into BCD and then storing each input to its respective RTC register. This requires that the interrupts be disabled first before performing any changes. Once the values are stored, the interrupts are enabled again.
   4. **Variables:**   
      int s\_time: the BCD results of each input that is used to store the information to the registers.
4. **getdate(int \*ptr):**-
   1. **Inputs:** int \*pointer
   2. **Outputs:** none
   3. **Description:** Grabs the year, month and day values from the RTC registers and stores them in the buffer. Similar to get\_Time(), this function takes the values that are in BCD and converts them to regular binary, where the buffer is then filled one digit at a time.
   4. **Variables:**  
      int I / int j: the int values that would split the BCD value in half, each being converted to binary to represent the actual value to be stored.
5. **setdate(int year, int month, int day):**-
   1. **Inputs:** int year, int month, int day
   2. **Outputs:** none
   3. **Description:** Changes the current date of the machine to the provided values. Similar to set\_Time(), this converts each input into BCD form before entering the values in the registers, after disabling the interrupts. Once it is done, the interrupts are enabled again.
6. **help():**-
   1. **Inputs:** none
   2. **Outputs:** none
   3. **Description:** Once invoked in Terminal, it simply displays available commands. The messages inform the user of what commands he/she is able to perform and what syntax or parameters are needed.
7. **version():**-
   1. **Inputs:** none
   2. **Outputs:** none
   3. **Description:** Once invoked, it will print a message informing the user of the version and release date of this OS.
8. **Polling(char\* buffer, int count):**-
   1. **Inputs:** char\* buffer, int count
   2. **Outputs:** number of characters entered (count)
   3. **Description:** Continuously checks for available data entered from the serial port by checking the status register’s least significant bit (register COM1+5). When data is available, it will be taken from the data register and be stored in the buffer, while increasing count for each alphanumerical letter inserted into the buffer. This builds the user input from the terminal into the buffer while also printing each character onto the screen. Polling also takes into consideration special keystrokes and performs special actions depending on what keys were pressed. It is called from commhand() whenever a task has been performed.
   4. **Variables:**  
      int i: used for indexing of the buffer.  
      int counter: an int data type storing the size of the buffer.
9. **Kmain():**-
   1. **Inputs:** none
   2. **Outputs:** none
   3. **Description:** Performs all the initialization steps needed before MPX is ready for the user. Starts by initializing the serial port and setting the correct module to use. Then it will initialize the descriptor tables and interrupt vector tables. Lastly, it will initialize paging before invoking commhand() for processing user commands until shutdown.
10. **print(char\* str, int size):-**
    1. **Inputs:** char\* str, int size
    2. **Outputs:** none
    3. **Description:** invokes an instance of sys\_req(WRITE,..) by using ‘str’ as the string to be printed and ‘size’ as the size of the string to be printed.
11. **itoa(int number, char\* str):**-
    1. **Inputs:** int number, char\* str
    2. **Outputs:** String representation of the number given
    3. **Description:** Creates an empty string and takes the number given. Performs a series of steps to convert the numbers into their equivalent ASCII codes (characters) and puts them in the string in reverse order. Using flip(), which in return invokes swap(), flips the string to the correct orientation before returning the string representation of the number.
    4. **Variables:**int isNegative: a flag to indicate whether the given number is positive or negative.  
       int temp: Stores the absolute value of the number (after indicating that its negative or positive)  
       int i: index of the string
12. **flip(char\* str, int length):-**
    1. **inputs:** char\* str, int length
    2. **outputs:** A flipped version of the provided string
    3. **description:** Given a string and its length, uses two indices at each end of the string. Traversing to the middle, each character at the index is switched with the other index’s character with the help of swap(). This results in a flipped version of the string. Once finished, it will return the flipped string.
    4. **Variables:**  
       int i/j: index variables.
13. **Swap(char \*a, char \*b):**-
    1. **Inputs:** char\* a/b
    2. **Outputs:** none
    3. **Description:** switches the contents of the two pointers with one another. Using a temp variable first, performs a number of switching to prevent loss of data.
    4. **Variables:**  
       char temp: temporarily stores a pointer’s content aside while switching is in progress.
14. **allocatePCB():**-
    1. **Inputs:** none
    2. **Outputs:** pcb pointer to new PCB.
    3. **Description:** uses sys\_alloc\_mem() to dynamically allocate enough memory for a new PCB. Also performs some initialization steps and gives some default values.
15. **setupPCB(char\* newname, unsigned char newClass, int newPriority):**-
    1. **Inputs:** char\* newname, unsigned char newClass, int newPriority
    2. **Outputs:** pcb pointer to new PCB.
    3. **Description:** invokes an instance of allocatePCB() and assigns it to a pointer. Using the given name, class, and priority, it will perform error checking to these values before assigning them to the newly created PCB.
16. **freePCB(pcb\* name):**-
    1. **Inputs:** pcb\* name
    2. **Outputs:** char\* cast of sys\_free\_mem()
    3. **Description:** dynamically deallocates the memory assigned for the PCB. This is used when trying to permanently delete the PCB from memory.
17. **findPCB(char\* name):**-
    1. **Inputs:** char\* name
    2. **Output:** pointer to a PCB of the given name, or NULL
    3. **Description:** Using the given name, it will look through all queues for any PCB with a name matching what’s provided. When found, it will return a pointer to that PCB. If it fails to find a PCB from any queue, it will return NULL.
    4. **Variables:**  
       pcb\* ptr: the pointer to be returned when finding the PCB.
18. **insertPCB(pcb\* pntr):**-
    1. **Inputs:** pcb\* pntr
    2. **Outputs:** none
    3. **Description:** Given a pcb pointer, it will look at its priority, state, and status, and then traverse through the correct queue and connect the pcb to the surrounding PCB’s in either priority or FIFO base.
19. **removePCB(pcb\* pntr):**-
    1. **Inputs:** pcb\* pntr
    2. **Outputs:** int indicating success or error
    3. **Description:** Given the pcb pointer, it will adjust connections to its next and previous pcbs and ensures that the queue remains intact after disconnecting the PCB.
20. **showPCB(pcb\* pntr):**-
    1. **Inputs:** pcb\* pntr
    2. **Outputs:** none
    3. **Description:** Given a pcb pointer, it will print to the terminal screen any relevant information about the PCB, such as name, class, state, status, and priority.
21. **showqueue(char\* queue):**-
    1. **Inputs:** char\* queue
    2. **Outputs:** none
    3. **Description:** based on what keyword is provided in the string, it will traverse through the appropriate queue and invokes showPCB() for each individual PCB. This allows for printing an entire queue easily.